From 70f8f689a152aee9a599c310a09da0a72508af6d Mon Sep 17 00:00:00 2001
From: Torbjörn Andersson
Date: Fri, 16 Jul 2004 10:24:29 +0000
Subject: Applied patch #957544 to make output sample rate configurable at
 runtime.

svn-id: r14225
---
 doc/08.tex | 2 ++
 1 file changed, 2 insertions(+)

(limited to 'doc/08.tex')

diff --git a/doc/08.tex b/doc/08.tex
index 0fd6dd7a6b..1d569a2e3f 100644
--- a/doc/08.tex
+++ b/doc/08.tex
@@ -92,6 +92,8 @@ The following keywords are recognized:
         joystick\_num   &number   Number of joystick device to use for input\\
         master\_volume  &number   The master volume setting (0-255)\\
         music\_driver   &string   The music engine to use.\\
+        output\_rate    &number   The output sample rate to use, in Hz. Sensible\\
+                        &         values are 11025, 22050 and 44100.\\
         alsa\_port      &string   Port to use for output when using the\\
                         &         ALSA music driver.\\
         music\_volume   &number   The music volume setting (0-255)\\
-- 
cgit v1.2.3

